*To measure current in this wire:*

*…and reconnect through the ammeter.*

*Break the circuit somehow…*

A