incident

beam

aperture wheel

positioning wheel

light

sensor

rail

gain

switch

rail stop

Detector

Assembly

*ROTARY MOTION*

*SENSOR*

GAIN

1

10

100

Multiple

Slit Set

wheel

with slits

Laser

adjustment

screws

power

switch

scattered

beam